VN100 Settings

We do not have full “sanctified” settings yet.

As near as I can tell the factor defaults are OK, except for:

1. Async Data Output Frequency needs to be changed to 10Hz
2. The VPE heading mode needs to be changed to ABSOLUTE
3. The magnetometer basic calibration should be set to Off, cal manual, and convergence rate 1

Here is a screen shot of the settings on MY vn100. I still need to xcheck what jeff was using.

